## **SP4-H0727-N**

**Technical Specifications**

|  |  |
| --- | --- |
| Frequency Range | 698~2700 MHz |
| Split Loss | ≤ 6.45 dB |
| VSWR | ≤1.3 |
| Impedance | 50 Ω |
| Power Handling | 200W |
| PIM3 | < -150dBc@2\*20W |
| Connector | N Female |
| Operating Temperature | -25~+60 °C |
| Relative Humidity | 0~95 % |
| Application | Indoor or Outdoor (IP65) |
| Dimensions | 226.4x52x38.5 mm |
| Port | 1 input ports + 4 output ports |
| Weight | ≤2kg |
| Inner Contact Plating | Silver |
| Outer Contact Plating | Silver |

**Drawing**

